---
id: devices
title: Devices | Supported Hardware Overview
description: Detailed documentation on Meshtastic supported devices, including hardware specifications, performance comparisons, and guides.
sidebar_label: Devices
sidebar_position: 1
---

## Supported Devices

Meshtastic firmware can be installed on a wide range of development boards. The list below provides a brief comparison of currently supported hardware.

### Which board should I choose?

While all the boards listed on this page will run Meshtastic and mesh with each other, some current community favorites are:

- RAK Meshtastic Start Kit: [RAK19007](/docs/hardware/devices/rak-wireless/wisblock/base-board/?rakbase=RAK19007)+[RAK4631](/docs/hardware/devices/rak-wireless/wisblock/core-module/?rakcore=RAK4631)
- [HELTEC LoRa V3](/docs/hardware/devices/heltec-automation/lora32/?heltec=v23)
- [Nano G2 Ultra](/docs/hardware/devices/b-and-q-consulting/nano/?nano-series=g2)
- [Station G2](/docs/hardware/devices/b-and-q-consulting/station-series/?station-series=g2)
- [LILYGO LoRa T3-S3](/docs/hardware/devices/lilygo/lora/?t-lora=S3-v1)

Please do your research and choose the board that meets your needs (or maybe already have in a bin somewhere).

:::info

- The Semtech SX1262 transceiver is newer than the SX1276 and provides increased receive and transmit performance.
- nRF52-based devices use a fraction of the power compared to ESP32-based devices and are therefore generally preferred for solar and handset applications.
- ESP32-based devices require more power to operate but are typically lower-cost alternatives that do perform well when using house power, or for handsets that only require a day or two of runtime, and for applications that require WiFi connectivity.

:::

## RAK®

### [Wisblock](./rak-wireless/wisblock/)

Modular hardware system with Base, Core and Peripheral modules including the low-power and solar ready nRF52840-based Meshtastic Starter Kit (19007 & 4631).

[**WisBlock Core Modules**](./rak-wireless/wisblock/core-module/)<br/>
| Name | MCU | Radio | WiFi | BT | GPS |
|:-----------------------------------------------|:---------|:-------|:------------:|:---:|:------:|
| [RAK4631](./rak-wireless/wisblock/core-module?rakcore=RAK4631) | nRF52840 | SX1262 | NO | 5.0 | add-on |
| [RAK11200](./rak-wireless/wisblock/core-module?rakcore=RAK11200) | ESP32 | add-on | 2.4GHz b/g/n | 4.2 | add-on |
| [RAK11310](./rak-wireless/wisblock/core-module?rakcore=RAK11310) | RP2040 | SX1262 | NO | NO | add-on |

[**Base Boards**](./rak-wireless/wisblock/base-board/)<br/>
[RAK5005-O](./rak-wireless/wisblock/base-board?rakbase=RAK5005-O)<br/>
[RAK19007](./rak-wireless/wisblock/base-board?rakbase=RAK19007)<br/>
[RAK19003](./rak-wireless/wisblock/base-board?rakbase=RAK19003)<br/>
[RAK19001](./rak-wireless/wisblock/base-board?rakbase=RAK19001)<br/>

[**WisBlock Displays**](./rak-wireless/wisblock/screens/)<br/>
[RAK1921](./rak-wireless/wisblock/screens?rakscreens=OLED)<br/>
[RAK1400](./rak-wireless/wisblock/screens?rakscreens=E-Ink)<br/>

[**WisBlock Peripherals**](./rak-wireless/wisblock/peripherals/)<br/>
[RAK1910](./rak-wireless/wisblock/peripherals?rakmodules=GPS) GPS<br/>
[RAK12500](./rak-wireless/wisblock/peripherals?rakmodules=GPS) GPS<br/>
[RAK18001](./rak-wireless/wisblock/peripherals?rakmodules=Buzzer) Buzzer<br/>
[RAK13002](./rak-wireless/wisblock/peripherals?rakmodules=IO) IO<br/>
RAK14001 RGB LED<br/>
[RAK12002](./rak-wireless/wisblock/peripherals?rakmodules=RTC) RTC<br/>
[RAK1901](./rak-wireless/wisblock/peripherals?rakmodules=Sensors&sensors=RAK1901) Temperature and Humidity Sensor<br/>
[RAK1902](./rak-wireless/wisblock/peripherals?rakmodules=Sensors&sensors=RAK1902) Barometric Pressure Sensor<br/>
[RAK1906](./rak-wireless/wisblock/peripherals?rakmodules=Sensors&sensors=RAK1906) Environment Sensor<br/>
RAK12013 Radar Sensor<br/>
RAK13800 Ethernet Module<br/>

## LILYGO®

### [T-Beam](./lilygo/tbeam/)

Boards complete with GPS, 18650 battery holder, and optional screen.

| Name                                            | MCU      | Radio             |     WiFi     | BT  | GPS |
| :---------------------------------------------- | :------- | :---------------- | :----------: | :-: | :-: |
| [T-Beam v0.7](./lilygo/tbeam/?t-beam=0.7)       | ESP32    | SX1276            | 2.4GHz b/g/n | 4.2 | YES |
| [T-Beam v1.1](./lilygo/tbeam/?t-beam=1.1)       | ESP32    | SX1276            | 2.4GHz b/g/n | 4.2 | YES |
| [T-Beam with M8N](./lilygo/tbeam/?t-beam=m8n)   | ESP32    | SX1276<br/>SX1262 | 2.4GHz b/g/n | 4.2 | YES |
| [T-Beam S3-Core](./lilygo/tbeam/?t-beam=s3core) | ESP32-S3 | SX1262            | 2.4GHz b/g/n | 5.0 | YES |
| [T-BeamSUPREME](./lilygo/tbeam/?t-beam=supreme) | ESP32-S3 | SX1262            | 2.4GHz b/g/n | 5.0 | YES |

### [T-Echo](./lilygo/techo/)

All-in-one unit with E-Ink screen, GPS and battery in injection-molded case. Features the low-power nRF52840 for long battery life.

| Name                      | MCU      | Radio  | WiFi | BT  | GPS |
| :------------------------ | :------- | :----- | :--: | :-: | :-: |
| [T-Echo](./lilygo/techo/) | nRF52840 | SX1262 |  NO  | 5.0 | YES |

### [LoRa](./lilygo/lora/)

Inexpensive basic ESP32-based boards.

| Name                                              | MCU      | Radio                        |     WiFi     | BT  | GPS |
| :------------------------------------------------ | :------- | :--------------------------- | :----------: | :-: | :-: |
| [LoRa32 V1](./lilygo/lora/?t-lora=v1)             | ESP32    | SX127x                       | 2.4GHz b/g/n | 4.2 | NO  |
| [LoRa32 V1.3](./lilygo/lora/?t-lora=v1.3)         | ESP32    | SX127x                       | 2.4GHz b/g/n | 4.2 | NO  |
| [LoRa32 V2.0](./lilygo/lora/?t-lora=v2.0)         | ESP32    | SX127x                       | 2.4GHz b/g/n | 4.2 | NO  |
| [LoRa32 V2.1-1.6](./lilygo/lora/?t-lora=v2.1)     | ESP32    | SX127x                       | 2.4GHz b/g/n | 4.2 | NO  |
| [LoRa32 V2.1-1.8](./lilygo/lora/?t-lora=v2.1-1.8) | ESP32    | SX1280                       | 2.4GHz b/g/n | 4.2 | NO  |
| [LoRa32 T3-S3 V1.0](./lilygo/lora/?t-lora=S3-v1)  | ESP32-S3 | SX1262<br/>SX1276<br/>SX1280 | 2.4GHz b/g/n | 5.0 | NO  |

### [T-Deck](./lilygo/tdeck/)

Standalone device with screen and keyboard

| Name                      | MCU         | Radio  | WiFi | BT  | GPS |
| :------------------------ | :---------- | :----- | :--: | :-: | :-: |
| [T-Deck](./lilygo/tdeck/) | ESP32-S3FN8 | SX1262 | YES  | 5.0 | NO  |

### [T-Watch S3](./lilygo/twatch/)

| Name                           | MCU      | Radio  | WiFi | BT  | GPS |
| :----------------------------- | :------- | :----- | :--: | :-: | :-: |
| [T-Watch S3](./lilygo/twatch/) | ESP32-S3 | SX1262 | YES  | 5.0 | NO  |

## HELTEC®

### [LoRa 32](./heltec-automation/lora32/)

Inexpensive basic ESP32-based boards.

| Name                                                                                | MCU         | Radio  |     WiFi     | BT  | GPS |
| :---------------------------------------------------------------------------------- | :---------- | :----- | :----------: | :-: | :-: |
| [LoRa32 V2.1](./heltec-automation/lora32/?heltec=v2.1)                              | ESP32       | SX127x | 2.4GHz b/g/n | 4.2 | NO  |
| [LoRa32 V3/3.1](./heltec-automation/lora32/?heltec=v23)                             | ESP32-S3FN8 | SX1262 | 2.4GHz b/g/n | 5.0 | NO  |
| [Wireless Stick Lite V3](./heltec-automation/lora32/?heltec=Wireless+Stick+Lite+V3) | ESP32-S3FN8 | SX1262 | 2.4GHz b/g/n | 5.0 | NO  |
| [Wireless Tracker v1.0](./heltec-automation/lora32/?heltec=tracker-v1.0)            | ESP32-S3FN8 | SX1262 | 2.4GHz b/g/n | 5.0 | YES |
| [Wireless Tracker v1.1](./heltec-automation/lora32/?heltec=tracker-v1.1)            | ESP32-S3FN8 | SX1262 | 2.4GHz b/g/n | 5.0 | YES |
| [Wireless Paper](./heltec-automation/lora32/?heltec=paper)                          | ESP32-S3FN8 | SX1262 | 2.4GHz b/g/n | 5.0 | NO  |

### [Plug & Play Sensors](./heltec-automation/sensor/)

| Name                                      | MCU         | Radio  | WiFi         | BT  | GPS |
| ----------------------------------------- | ----------- | ------ | ------------ | --- | --- |
| [Capsule V3](./heltec-automation/sensor/) | ESP32-S3FN8 | SX1262 | 2.4GHz b/g/n | 5.0 | YES |

### [Vision Master](./heltec-automation/vision-master/)

Versatile ESP32-S3-based boards E-Ink development boards.

| Name                                                                               | MCU        | Radio  |     WiFi     | BT  | GPS |
| :--------------------------------------------------------------------------------- | :--------- | :----- | :----------: | :-: | :-: |
| [Vision Master E213](./heltec-automation/vision-master/?heltec=vision_master_e213) | ESP32-S3R8 | SX1262 | 2.4GHz b/g/n | 5.0 | NO  |
| [Vision Master E290](./heltec-automation/vision-master/?heltec=vision_master_e290) | ESP32-S3R8 | SX1262 | 2.4GHz b/g/n | 5.0 | NO  |
| [Vision Master T190](./heltec-automation/vision-master/?heltec=vision_master_t190) | ESP32-S3R8 | SX1262 | 2.4GHz b/g/n | 5.0 | NO  |

## [B&Q Consulting](./b-and-q-consulting/)

### [Nano Series](./b-and-q-consulting/nano/)

Portable and durable devices designed for Meshtastic.

| Name                                                            | MCU         | Radio  |     WiFi     | BT  | GPS |
| :-------------------------------------------------------------- | :---------- | :----- | :----------: | :-: | :-: |
| [Nano G2 Ultra](./b-and-q-consulting/nano/?nano-series=g2)      | NRF52840    | SX1262 | 2.4GHz b/g/n | 5.0 | YES |
| [Nano G1 Explorer](./b-and-q-consulting/nano/?nano-series=g1-e) | ESP32 WROOM | SX1262 | 2.4GHz b/g/n | 4.2 | YES |
| [Nano G1](./b-and-q-consulting/nano/?nano-series=g1)            | ESP32 WROOM | SX1276 | 2.4GHz b/g/n | 4.2 | YES |

### [Station Series](./b-and-q-consulting/station-series/)

High power LoRa transceiver designed for Meshtastic Licensed HAM operation.

| Name                                               | MCU              | Radio  |     WiFi     | BT  |   GPS    |
| :------------------------------------------------- | :--------------- | :----- | :----------: | :-: | :------: |
| [Station G1](./b-and-q-consulting/station-series/) | ESP32 WROOM      | SX1262 | 2.4GHz b/g/n | 4.2 | OPTIONAL |
| [Station G2](./b-and-q-consulting/station-series/) | ESP32-S3 WROOM-1 | SX1262 | 2.4GHz b/g/n | 5.0 | OPTIONAL |

## [Raspberry Pi](./raspberrypi/)

### [Raspberry Pi Pico](./raspberrypi/pico/)

Fast versatile boards using the RP2040.

| Name                                    | MCU    | Radio  |     WiFi     |      BT       | GPS |
| :-------------------------------------- | :----- | :----- | :----------: | :-----------: | :-: |
| [Raspberry Pi Pico](./raspberrypi/pico) | RP2040 | SX1262 | 2.4GHz b/g/n | not supported | NO  |

[**Pico Peripherals**](./raspberrypi/pico/peripherals/)<br/>
SSD1306 OLED Display<br/>
SH1106 OLED Display<br/>
CardKB Keyboard<br/>

### [Raspberry Pi Zero/Zero2/3/4/400/5](./linux-native-hardware/)

Meshtastic offers support for Raspberry Pi devices through our Linux native platform, meshtasticd. For full information, please see our [Linux Native Hardware](./linux-native-hardware/) documentation.

## Seeed Studio

### SenseCap

The SenseCAP product line offers a comprehensive range of solutions for both hobbyists and industrial users, featuring the T1000-E card tracker, an IP65-rated, ready-to-go Meshtastic device, and the Indicator with a 4-inch touchscreen driven by ESP32-S3 and RP2040 Dual-MCU, coming soon.

| Name                                                          | MCU           | Radio  | WiFi | BT  | GPS |
| ------------------------------------------------------------- | ------------- | ------ | ---- | --- | --- |
| [Card Tracker T1000-E](./seeed-studio/sensecap/card-tracker/) | nRF52840      | LR1110 | NO   | 5.1 | YES |
| [SenseCAP Indicator](./seeed-studio/) (coming soon)           | ESP32, RP2040 | -      | -    | -   | -   |

### [Seeed Wio-WM1110](./seeed-studio/wm1110)

nRF52840-based development boards with GPS, and multiple ports to attach sensors.

| Name                                                                      | MCU      | Radio  | WiFi | BT  | GPS |
| :------------------------------------------------------------------------ | :------- | :----- | :--: | :-: | :-: |
| [Seeed Wio-WM1110 Dev Kit](./seeed-studio/wm1110?wm1110=wio-sdk-wm1110)   | nRF52840 | LR1110 | YES  | 5.3 | YES |
| [Seeed Wio Tracker 1110](./seeed-studio/wm1110?wm1110=wio-tracker-wm1110) | nRF52840 | LR1110 | YES  | 5.3 | YES |

## [CanaryOne](./canary)

Complete solution with battery, screen, case, and antenna. Ships pre-flashed with latest Meshtastic firmware.

| Name                  | MCU      | Radio  | WiFi | BT  | GPS |
| :-------------------- | :------- | :----- | :--: | :-: | :-: |
| [CanaryOne](./canary) | nRF52840 | SX1262 |  NO  | 5.0 | YES |

## [unPhone](./unPhone)

All-in-one development device with LoRa, WiFi, BT, touchscreen, accelerometer, gyroscop, vibration motor, LiPo battery and more!

| Name                 | MCU              | Radio  | WiFi | BT  | GPS |
| :------------------- | :--------------- | :----- | :--: | :-: | :-: |
| [unPhone](./unPhone) | ESP32-S3-WROOM-1 | RF950W | YES  | 5.0 | NO  |

### [Seeed Wio-WM1110](./seeed-studio/wm1110)

nRF52840-based development boards with GPS, and multiple ports to attach sensors.

| Name                                                                      | MCU      | Radio  | WiFi | BT  | GPS |
| :------------------------------------------------------------------------ | :------- | :----- | :--: | :-: | :-: |
| [Seeed Wio-WM1110 Dev Kit](./seeed-studio/wm1110?wm1110=wio-sdk-wm1110)   | nRF52840 | LR1110 | YES  | 5.3 | YES |
| [Seeed Wio Tracker 1110](./seeed-studio/wm1110?wm1110=wio-tracker-wm1110) | nRF52840 | LR1110 | YES  | 5.3 | YES |

## [Chatter](./chatter)

DIY kit with ESP32, LoRa chip, and optional GPS. Designed for STEM education.

| Name                 | MCU   | Radio  | WiFi | BT  | GPS |
| :------------------- | :---- | :----- | :--: | :-: | :-: |
| [Chatter](./chatter) | ESP32 | LLCC68 | YES  | 4.2 | No  |

### Radio Master

| Name                  | MCU              | Radio  | WiFi | BT  | GPS |
| :-------------------- | :--------------- | :----- | :--: | :-: | :-: |
| Bandit Nano ExpressLRS 900 | ESP32 | SX1276 + SKY66122 PA/LNA +30db TX, +16db RX ) | ?  | YES | NO  |
