---
id: nrf52
title: nRF52/RP2040 Serial Drivers
sidebar_label: nRF52/RP2040 Drivers
sidebar_position: 2
description: Instructions for installing nRF52 and RP2040 USB serial drivers to interact with a Meshtastic device.
---

import Tabs from "@theme/Tabs";
import TabItem from "@theme/TabItem";
import Link from "@docusaurus/Link";

## Install nRF52/RP2040 USB to Serial Drivers

:::caution

nRF52/RP2040 devices typically do not require serial drivers. They use the UF2 bootloader which makes the devices appear as flash drives.  Do _NOT_ download the USB device drivers unless required to install UF2 support.

:::

<Tabs
groupId="operating-system"
defaultValue="windows"
values={[
{label: 'Linux', value: 'linux'},
{label: 'macOS', value: 'macos'},
{label: 'Windows', value: 'windows'},
]}>

<TabItem value="linux">

#### Linux

- [CH34x Driver - Linux Download](http://www.wch-ic.com/downloads/CH341SER_LINUX_ZIP.html)

</TabItem>

<TabItem value="macos">

#### macOS

:::info

With the latest versions of MacOS, the USB Serial driver is built-in. If you downloaded/installed any already, please remove them.

:::

##### Remove the CH34x USB Driver (macOS)

If you have already downloaded/installed the macOS WCH-IC CH340/CH341
("CH341SER_MAC") drivers via the CH34x_Install_V1.5.pkg, you will have to
Uninstall the kernel extension:

1. Unplug your device
2. Open the Terminal and run:
3. `sudo rm -rf /Library/Extensions/usbserial.kext`
4. Reboot


##### Install the CH34x Driver

- [CH34x Driver- macOS Download](https://github.com/WCHSoftGroup/ch34xser_macos)



</TabItem>

<TabItem value="windows">

#### Windows

- [CH34x Driver - Windows Download](http://www.wch-ic.com/downloads/CH341SER_EXE.html)

</TabItem>

</Tabs>

:::important

After installing the driver, make sure to reboot your computer to finish the installation process.

You can also [test your serial driver installation](/docs/getting-started/serial-drivers/test-serial-driver-installation) at this step if required.

:::

### Flash Firmware

After installing the serial drivers, you can now flash the Meshtastic firmware onto your device. To proceed, select the appropriate device type for your device.

<div className="indexCtasBody">
  <Link
    className={"button button--outline button--lg cta--button"}
    to={"/docs/getting-started/flashing-firmware/nrf52/"}
  >
    Flash nRF52/RP2040 Firmware
  </Link>
</div>
