---
id: network
title: Network Configuration
sidebar_label: Network
description: Learn about network configuration for your Meshtastic device including NTP, WiFi, and Ethernet.
---

import Tabs from "@theme/Tabs";
import TabItem from "@theme/TabItem";

The Network config options are: NTP Server, WiFi Enabled, WiFi SSID, WiFi PSK, Ethernet Enabled, IPv4 Networking Mode, and Static Address. Network config uses an admin message sending a `Config.Network` protobuf.

:::info
Enabling WiFi will disable Bluetooth. Only one connection method will work at a time.
:::

ESP32 devices have the ability to connect to WiFi as a client. SoftAP mode is not supported by the Meshtastic firmware.

## Network Config Values

### NTP Server

The NTP server used if IP networking is available.

Set to `0.pool.ntp.org` by default. (Max Length: 32)

### WiFi Enabled

Enables or Disables WiFi.

Set to `false` (Disabled) by default.

### WiFi SSID

This is your WiFi Network's SSID.

Empty `""` by default. (Case Sensitive, Max Length: 32)

### WiFi PSK

This is your WiFi Network's password.

Empty `""` by default. (Case Sensitive, Max Length: 64)

### Ethernet Enabled

Enables or Disables Ethernet.

Set to `false` (Disabled) by default.

### IPv4 Networking Mode

Set to `DHCP` by default. Change to `STATIC` to use a static IP address. Applies to both Ethernet and WiFi.

### IPv4 Static Address configuration

contains ip, gateway, subnet and dns server in case you want a static configuration.

:::tip
The first time your device restarts after enabling WiFi or Ethernet, it will take an additional 20-30 seconds to boot. This is to generate self-signed SSL keys. The keys will be saved for future reuse.
:::

## Network Config Client Availability

<Tabs
groupId="settings"
defaultValue="cli"
values={[
{label: 'Android', value: 'android'},
{label: 'Apple', value: 'apple'},
{label: 'CLI', value: 'cli'},
{label: 'Web', value: 'web'},
]}>

<TabItem value="android">

#### Android

:::info

Network Config options are available for Android.

1. Open the Meshtastic App
2. Navigate to: **Vertical Ellipsis (3 dots top right) > Radio Configuration > Network**

:::

</TabItem>

<TabItem value="apple">

#### Apple

:::info

All Network config options are available on iOS, iPadOS and macOS at Settings > Device Configuration > Network.

:::

</TabItem>

<TabItem value="cli">

#### CLI

:::info

All Network config options are available in the python CLI.

:::

|       Setting        | Acceptable Values |     Default      |
| :------------------: | :---------------: | :--------------: |
|  network.ntp_server  |      string       | `0.pool.ntp.org` |
| network.wifi_enabled |  `true`, `false`  |     `false`      |
|  network.wifi_ssid   |      string       |       `""`       |
|   network.wifi_psk   |      string       |       `""`       |
| network.eth_enabled  |  `true`, `false`  |     `false`      |
| network.address_mode | `DHCP`, `STATIC`  |      `DHCP`      |

:::tip

Because the device will reboot after each command is sent via CLI, it is recommended when setting multiple values in a config section that commands be chained together as one.

```shell title="Example:"
meshtastic --set network.wifi_enabled true --set network.wifi_ssid "my network" --set network.wifi_psk mypassword
```

:::

```shell title="Set NTP Server"
meshtastic --set network.ntp_server "0.pool.ntp.org"
```

```shell title="Enable / Disable WiFi"
meshtastic --set network.wifi_enabled true
meshtastic --set network.wifi_enabled false
```

```shell title="Set WiFi SSID"

meshtastic --set network.wifi_ssid mynetwork
// With spaces
meshtastic --set network.wifi_ssid "my network"
```

```shell title="Set WiFi password"
meshtastic --set network.wifi_psk mypassword
// With spaces
meshtastic --set network.wifi_psk "my password"
```

</TabItem>

<TabItem value="web">

#### Web

:::info
All Network config options are available in the Web UI.
:::

</TabItem>

</Tabs>

## Examples

### WiFi Client

With `network.wifi_ssid` & `network.wifi_psk` populated, the device will know to connect to your network. Make sure you are in range of your WiFi and it is a 2.4GHz-only network. If you have a single Meshtastic device on your local network it's easy to connect to your device with DNS `http://meshtastic.local`. If you have multiple Meshtastic devices you will need to connect using their respective IP addresses.

### Disable WiFi

To disable WiFi completely, set `network.wifi_enabled` to `false`.
