---
id: wisBlock
title: RAK WisBlock
sidebar_label: RAK WisBlock
sidebar_position: 3
---

import Tabs from '@theme/Tabs';
import TabItem from '@theme/TabItem';

The RAK WisBlock is a low power modular hardware system that can be used to build Meshtastic devices. Soldering is only required for the optional OLED screen.

RAK Wireless currently sell a [Meshtastic Starter kit](https://store.rakwireless.com/products/wisblock-meshtastic-starter-kit) that has the minimum you need to get started. If you wish to purchase parts separately, you will need a [base board](https://store.rakwireless.com/collections/wisblock-base), a [core 4631 LPWAN module](https://store.rakwireless.com/collections/wisblock-core/products/rak4631-lpwan-node), and optionally a GPS Sensor, scrren or other module to build a Meshtastic device. Please ensure you choose the correct operating frequency for your country when purchasing.

Please see the RAK documentation for the correct way to connect your hardware to ensure that you do not damage the device. There is currently no pin required to pair RAK devices via BLE.

## RAK base boards
<Tabs
groupId="rakbase board"
defaultValue="RAK5005-O"
values={[
{label: 'RAK5005-O', value: 'RAK5005-O'},
{label: 'RAK19003', value: 'RAK19003'},
{label: 'RAK19001', value: 'RAK19001'},
{label: 'RAK19007', value:'RAK19007'}
]}>
<TabItem value="RAK5005-O">

[RAK5005-O](https://store.rakwireless.com/products/rak5005-o-base-board) - The original WisBlock Base Board

- Reset button 
- OLED screen support (OLED screen sold separately)
- Connector for 3.7v LiPo battery (with charge controller)
- Connector for 5v solar panel (max 5.5v)
- 1x Core Module slot
- 1x WisBlock IO Module slot
- 4x WisBlock Sensor Module slots
- I2C, UART, GPIOs and analog input accessible with solder contacts
- Micro USB port for debugging and power


Further information on the RAK5005-O can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK5005-O/Overview/#product-description).

It may be possible to add a user button using the [13002 IO module](https://store.rakwireless.com/collections/wisblock-interface/products/adapter-module-rak13002).

- [Update the bootloader](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK4631/Quickstart/#updating-the-bootloader) on first use! This can be done easily with [Meshtastic-flasher](https://github.com/meshtastic/Meshtastic-gui-installer)
- Firmware for 5005 base board: [`firmware-rak4631_5005-1.x.x.uf2`](/downloads) 


  <img
    alt="RAK4631 5005"
    src="/img/hardware/rak4631_5005.png"
    style={{ zoom: '50%' }}
  />

</TabItem>
<TabItem value="RAK19003">

[RAK19003](https://store.rakwireless.com/products/wisblock-base-board-rak19003) - WisBlock Mini Base Board

- Reset button 
- OLED screen support (OLED screen sold separately)
- Connector for 3.7v LiPo battery (with charge controller)
- Connector for 5v solar panel (max 5.5v)
- 1x Core Module slot
- 2x WisBlock Sensor Module slots
- I2C, UART and BOOT headers accessible with solder contacts
- Micro USB port for debugging and power


Further information on the RAK19003 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK19003/Overview/#product-description).

It is currently not possible to add a user button to this board.

- Firmware for 19003 base board: [`firmware-rak4631_19003-1.x.x.uf2`](/downloads)

  <img
    alt="RAK4631 19003"
    src="/img/hardware/rak4631_19003.png"
    style={{ zoom: '50%' }}
  />

</TabItem>
<TabItem value="RAK19001">

[RAK19001](https://store.rakwireless.com/products/rak19001-wisblock-dual-io-base-board) - WisBlock Dual IO Base Board

:::caution
This board should work with the RAK5005-O firmware, however this is currently uncomfirmed.
:::

- Reset and user definable buttons
- OLED screen support (OLED screen sold separately)
- Connector for 3.7v LiPo battery (with charge controller)
- Separate connector for non-rechargeable batteries
- Connector for 5v solar panel (max 5.5v)
- 1x Core Module slot
- 2x WisBlock IO Module slot
- 6x WisBlock Sensor Module slots
- I2C, SPI, UART, BOOT and GPIOs accessible with solder contacts
- USB-C port for debugging and power
- Battery selector switch


Further information on the RAK19001 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK19001/Overview/#product-description).

It may be possible to add a user button using the [13002 IO module](https://store.rakwireless.com/collections/wisblock-interface/products/adapter-module-rak13002).

</TabItem>
<TabItem value="RAK19007">

[RAK19007](https://store.rakwireless.com/products/rak19007-wisblock-base-board-2nd-gen) - WisBlock Base Board - 2nd Generation  
This is an upgrade to the original RAK5005-O base board.

:::caution
This board should work with the RAK5005-O firmware, however this is currently uncomfirmed.
:::

- Reset button 
- OLED screen support (OLED screen sold separately)
- Connector for 3.7v LiPo battery (with charge controller)
- Connector for 5v solar panel (max 5.5v)
- 1x Core Module slot
- 1x WisBlock IO Module slot
- 4x WisBlock Sensor Module slots
- I2C, UART, BOOT and GPIOs accessible with solder contacts
- USB-C port for debugging and power


Further information on the RAK19007 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK19007/Overview/#product-description).

It may be possible to add a user button using the [13002 IO module](https://store.rakwireless.com/collections/wisblock-interface/products/adapter-module-rak13002).

</TabItem>
</Tabs>

Flashing the firmware is a simple process. Connect your device via USB, click the reset button twice, and a drive will appear. On Windows, Linux, or Mac, drag the appropriate .uf2 firmware file onto the root of the drive and the firmware will be updated. Or, you can use [Meshtastic-flasher](https://github.com/meshtastic/Meshtastic-gui-installer). RAK have also provided [Installation instructions](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK4631/Quickstart/#rak4631-lora-mesh-via-meshtastic) for Meshtastic.


## Core Module

There are two core modules supported by Meshtastic:

<Tabs
groupId="rakcore"
defaultValue="RAK4631"
values={[
{label: 'RAK4631', value: 'RAK4631'},
{label: 'RAK11200', value: 'RAK11200'}
]}>
<TabItem value="RAK4631">

The main supported code is the [WisBlock LPWAN Module RAK4631](https://store.rakwireless.com/products/rak4631-lpwan-node).  
(Please note this is different to the RAK4631-R which uses different firmware incompatible with Meshtastic).

- nRF52840 microprocessor - Bluetooth BLE 5.0 and very low power consumption
- SX1262 - LoRa transceiver
- Frequency options:
  - 433 MHz
  - 470 MHz
  - 799 MHz
  - 865 MHz
  - 868 MHz
  - 915 MHz
  - 920 MHz
  - 923 MHz
- U.FL antenna connector


<img
  alt="RAK4631 Core Module"
  src="/img/hardware/rak4631.png"
  style={{ zoom: '50%' }}
/>

Further information on the RAK4631 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK4631/Overview/#product-description).

</TabItem>
<TabItem value="RAK11200">

The [RAK11200](https://store.rakwireless.com/products/wiscore-esp32-module-rak11200) is currently only supported on the RAK5005-O base board. This provides the benefits of WiFi, but sacrifices the very low power consumption of the nRF microprocessor used on the RAK4631.

- ESP32-WROVER microprocessor - Bluetooth 4.2 & WiFi 802.11 b/g/n

Further information on the RAK11200 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK11200/Overview/#product-description).

The RAK11200 does not contain a LoRa transceiver, and this needs to be added separately in the form of the [RAK13300 LPWAN module](https://store.rakwireless.com/products/rak13300-wisblock-lpwan). This occupies the IO Port of the base board.

The RAK13300 has the following specifications:
- SX1262 - LoRa transceiver
- Frequency options:
  - 433 MHz
  - 470 MHz
  - 864 MHz
  - 865 MHz
  - 868 MHz
  - 915 MHz
  - 920 MHz
  - 923 MHz
- U.FL antenna connector


Further information on the RAK13300 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK13300/Overview/#product-description).

- Firmware for 5005 with 11200: [`firmware-11200-1.3.x.bin`](/downloads)

  <img
    alt="RAK4631 5005 11200"
    src="/img/hardware/rak11200.jpg"
    style={{ zoom: '50%' }}
  />

</TabItem>
</Tabs>

## Screens

There are currently two different screens supported by the RAK WisBlock system:

<Tabs
groupId="rakscreens"
defaultValue="OLED"
values={[
{label: 'OLED Display', value: 'OLED'},
{label: 'E-Ink Display', value: 'E-Ink'}
]}>
<TabItem value="OLED">

The [RAK1921 OLED display](https://store.rakwireless.com/products/rak1921-oled-display-panel) is a 0.96 inch monocrome display.

- 0.96 inch OLED display
- Resolution 128 x 64 pixels
- I2C interface


This item requires soldering.  
Further information on the RAK1921 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK1921/Overview/#product-description).  
Similar modules are widely available from other suppliers, but do check the boards as some have the VDD and GND pins swapped round.

[<img alt="0.96 inch OLED display" src="/img/hardware/screen.png" style={{zoom:'25%'}} />](/img/hardware/screen.png)

</TabItem>
<TabItem value="E-Ink">

The [RAK1400 EPD module](https://store.rakwireless.com/products/wisblock-epd-module-rak14000) is an ultra low power E-Ink display with three user buttons.

- 2.13 inch black and white E-Ink display
- Three button module
- Resolution 212 x 104 pixels
- Occupies the IO Port of a Wisblock Base


- Firmware for 5005 with RAK14000 epaper: [`firmware-rak4631_19003-epaper-1.3.x.uf2`](/downloads)

  <img
    alt="RAK4631 5005 14000"
    src="/img/hardware/rak4631_5005_epaper.jpg"
    style={{ zoom: '50%' }}
  />

Please note only the white-black display is supported at this time, the white-black-red display may work, but is not supported.  
Further information on the RAK14000 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK14000/Overview/#product-description).

</TabItem>
</Tabs>

## Supported modules

<Tabs
groupId="rakmodules"
defaultValue="GPS"
values={[
{label: 'GPS Module', value: 'GPS'},
{label: 'Buzzer', value: 'Buzzer'},
{label: 'I/O Module', value: 'IO'},
{label: 'Environmental Sensor', value:'BME680'}
]}>
<TabItem value="GPS">

To add a GPS to the RAK5005-O base board, you need the [RAK1910 GPS sensor](https://store.rakwireless.com/collections/wisblock-sensor/products/rak1910-max-7q-gnss-location-sensor). It is supported on slot A of the 5005 board via UART.

- uBlox MAX-7Q GPS module
- GPS and GLONASS satelite support


Further information on the RAK1910 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK1910/Overview/#product-description).

To add a GPS to the RAK19003 base board, you need the [RAK12500 GPS sensor](https://store.rakwireless.com/products/wisblock-gnss-location-module-rak12500). It is supported via I2C on slot B for firmware versions 1.49 and above.

- uBlox Zoe-M8Q GNSS receiver
- GPS, GLONASS, QZSS and BeiDou satelite support


Further information on the RAK12500 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK12500/Overview/#product-description).

</TabItem>
<TabItem value="Buzzer">

The [RAK18001 Buzzer Module](https://store.rakwireless.com/products/wisblock-buzzer-module-rak18001) is currently being tested for integration with the External Notifications plugin. There is currently a known conflict with buzzer if the module is placed in Slot D, although other slots should work.

Further information on the RAK18001 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK18001/Overview/#product-description).

</TabItem>
<TabItem value="IO">

The [RAK13002 IO Module](https://store.rakwireless.com/collections/wisblock-interface/products/adapter-module-rak13002) can be used to, amongst other things, add a user button to the RAK base boards (excluding the RAK19003 Mini base board). It features a number of different interface options:

- 2x I2C interfaces
- 2x UART interfaces
- 1x SPI interface
- Upto 6x GPIOs
- 2x ADC interfaces
- 3.3v Power rails


There is development activity in progress to get sensors such as this added to the Meshtastic Core.  
Further information on the RAK13002 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK13002/Overview).

</TabItem>
<TabItem value="BME680">

The [RAK1906 Environmental Sensor](https://store.rakwireless.com/products/rak1906-bme680-environment-sensor) is based on the Bosch BME680 module and has the following features:

- Temperature measurement (Range -40&deg;C to +85&deg;C)
- Humidity measurement (Range 0% to 100%)
- Barometer measurement (Range 300 to 1100 hPa)
- Air Quality measurement


There is development activity in progress to get sensors such as this added to the Meshtastic Core.  
Further information on the RAK1906 can be found on the [RAK Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock/RAK1906/Overview/#product-description).

</TabItem>
</Tabs>

## RAK Wireless' Resources

- RAK's Wisblock [Documentation Center](https://docs.rakwireless.com/Product-Categories/WisBlock)
- RAK's [GitHub Page](https://github.com/RAKWireless/WisBlock) for the WisBlock