---
id: canaryone
title: CanaryOne
sidebar_label: Canary
sidebar_position: 12
---


The CanaryOne was built by Canary Radio Company from the ground up to run Meshtastic in austere environments as an affordable tactical networking solution.

CanaryOne custom PCB and case were designed and are assembled and manufactured in the United States.

The custom PCB board supports jlink debugging, with intelligent electrical components sourced from the United States and Western Europe. 

![CanaryOneFront](/img/hardware/canary-one/front.webp)

## Specifications

- **MCU**
  - NRF52840 (Bluetooth)
    - Bluetooth 5.0
- **LoRa Transceiver**
  - Semtech SX1262
- **Frequency options**
  - All Meshtastic options.
- **Navigation Module**
  - ATGM336H-5N-71 (Supports GPS, BDS and GLONASS)
- **Antenna**
  - SMA Socket
- **Connectors**
  - USB-C

## Resources

- Firmware file: `canary-one-X.X.X.xxxxxxx.bin`
- Purchase Link: [canaryradio.io](https://canaryradio.io/products/canaryone)

## Perspective Photos

![CanaryOnePerspective](/img/hardware/canary-one/perspective.webp)
![CanaryOneDos](/img/hardware/canary-one/dos.webp)
