---
id: screens
title: T-Beam Screens
sidebar_label: Screens
sidebar_position: 2
---

## 0.96 inch OLED I<sup>2</sup>C display

### Pin map

To attach the screen:

1. Connect VCC to 3v3
2. Connect GND to GND
3. Connect SCL to pin 22
4. Connect SDA to pin 21

![Connecting the OLED screen to a T-Beam](/img/hardware/t-beam-screen.webp)

### Resources
- Purchase Links:
  - US
    - [Rokland](https://store.rokland.com/products/lilygo-ttgo-0-96-inch-oled-white-color-text-display-module-l206-for-t-beam-and-t-sim)
  - International
    - [Aliexpress](https://www.aliexpress.com/item/32922106384.html)

![0.96 inch OLED display](/img/hardware/screen.webp)
