---
id: buttons
title: Nano Series Hardware Buttons
sidebar_label: Buttons
sidebar_position: 1
---

import Tabs from "@theme/Tabs";
import TabItem from "@theme/TabItem";

## Device

<Tabs
groupId="nano-series"
defaultValue="g2"
values={[
{label: 'Nano G2 Ultra', value:'g2'},
{label: 'Nano G1 Explorer', value: 'g1-e'},
{label: 'Nano G1', value: 'g1'}
]}>

<TabItem value="g2">

### Nano G2 Ultra

#### Buttons

- **User/Program Button:**
  - **Single press:** Changes the information page displayed on the device's screen.
  - **Double press:** Sends an adhoc ping of the device's position to the network.
  - **Long press:** Will signal the device to shutdown after 5 seconds (*soft off*).
- **Message Read Button:**
  - **Single press:** Clears the New Message LED.

#### Switches

- **Power:**
  - **Toggle Up:** Turns on the device.
  - **Toggle Down:** Turns off the device.
- **Location Pin:**
  - **Toggle Up:** Sets GPS to operating mode.
  - **Toggle Down:** Sets GPS to low power mode.
- **Bell:**
  - **Toggle Up:** Selects Buzzer for Enhanced Message Notification Circuit.
  - **Toggle Down:** Selects LED for Enhanced Message Notification Circuit.


</TabItem>
 <TabItem value="g1-e">

### Nano G1 Explorer

#### Buttons

- **User/Program Button:**
  - **Single press:** Changes the information page displayed on the device's screen.
  - **Double press:** Sends an adhoc ping of the device's position to the network.
- **Message Read Button:**
  - **Single press:** Clears the New Message LED.

### Switches

- **Power:**
  - **Toggle Up:** Turns on the device.
  - **Toggle Down:** Turns off the device.
- **Location Pin:**
  - **Toggle Up:** Sets GPS to operating mode.
  - **Toggle Down:** Sets GPS to low power mode.
- **Bell:**
  - **Toggle Up:** Selects Buzzer for Enhanced Message Notification Circuit.
  - **Toggle Down:** Selects LED for Enhanced Message Notification Circuit.

</TabItem>
<TabItem value="g1">



</TabItem>
</Tabs>
