---
id: station-g1
title: Station G1 device
sidebar_label: Station G1
sidebar_position: 9
---

The Station G1 is the second dedicated hardware device to be designed from scratch purely for Meshtastic Licensed (HAM) Operation by Neil Hao. It has been designed to be small and compact with the inclusion of 35dBm high power PA.

## Specifications

- **MCU**
  - ESP32 WROOM (WiFi & Bluetooth)
    - Bluetooth 4.2
- **LoRa Transceiver**
  - Semtech SX1262
  - Additional 35dBm LoRa Power Amplifier to boost transmit power
- **Frequency options**
  - US-915 MHz
  - EU-868 MHz
- **Navigation Module**
  - ATGM336H-5N-71 (Supports GPS, BDS and GLONASS)
- **Antenna**
  - SMA Socket
- **Connectors**
  - USB-C

## Features

- Meshtastic pre-installed
- User button
- 1.3 inch OLED screen
- Optional GPS Module and IO Extension Socket
- Optional [12V Battery Docker](https://shop.uniteng.com/product/12v-battery-docker-for-station-edition-g1/) which can be used as Backup Power, or in scenarios that require mobility

## Resources

- Firmware file: `firmware-station-g1-X.X.X.xxxxxxx.bin`
- [Unit Engineering's Official Wiki](https://uniteng.com/wiki/doku.php?id=meshtastic:station)
- Purchase Links:
  - International
    - [Official Store](https://shop.uniteng.com/product/meshtastic-mesh-device-station-edition/)
    - [Official Tindie Store](https://www.tindie.com/products/neilhao/meshtastic-mesh-device-station-edition/)

![Station G1](/img/hardware/station-g1.webp)
